{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["附表1询价表（需"],"read":"whole","date_system":"1900"}

{"sheet":"附表1询价表（需","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"merged":[[0,0,0,6],[1,0,1,6],[3,0,14,0],[3,1,14,1],[3,6,14,6],[15,0,21,0],[15,1,21,1],[15,6,21,6],[22,0,25,0],[22,1,25,1],[22,6,25,6],[28,0,28,1]]}
["合江县农业开发投资（集团）有限公司\n污水处理厂第三方水质检测询价项目报价表"]
["报价单位（盖章）：                                                                                                       年      月     日"]
["序号","检测项目","指标","年检测频次","单价","总价","备注"]
[1,"排水口常规项 \n（12 项）","化学需氧量",37,null,null,"每次检测采集瞬时水样\n至少三个瞬时样"]
[null,null,"氨氮",37]
[null,null,"总磷",37]
[null,null,"总氮",37]
[null,null,"pH值",37]
[null,null,"五日生化需氧量",37]
[null,null,"悬浮物",37]
[null,null,"色度",37]
[null,null,"动植物油",37]
[null,null,"粪大肠菌群",37]
[null,null,"石油类",37]
[null,null,"阴离子表面活性剂",37]
[2,"排水口重金属 离子\n（7项）","总汞",22,null,null,"每次检测采集瞬时水样\n至少三个瞬时样"]
[null,null,"总镉",22]
[null,null,"总铭",22]
[null,null,"总铅",22]
[null,null,"总砷",22]
[null,null,"六价铭",22]
[null,null,"烷基汞",22]
[3,"废气\n（4项）","氨",18,null,null,"每次检测要求非连续采样\n至少三次"]
[null,null,"臭气",18]
[null,null,"硫化氢",18]
[null,null,"甲烷",9]
[4,"噪声","厂界环境噪声",18,null,null,"昼间、夜间分别测定"]
[5,"污泥","污泥含水率",12,null,null,"每次检测采集三个点位样品"]
["总计："]